**Face Panel and Displays**

[Shift] + [Escape]

To lock and unlock face panel

[Escape] + [Encoder Page Keys]

Locks the encoders. Pressing any encoder page button unlocks.

[Encoder Page Key] + [Number]

Pages to the desired encoder control page

[Shift] + [Tab]

To close all tabs except Live/Blind and Playback Status

[Shift] + [Format]

Blind spreadsheet – expose/suppress non-intensity parameters (Element)

[Shift] + [Live/Blind]

Advances the displays to the next instance of live or blind.

[Live] – when already in live

Resyncs the selected cue to the most recently activated cue.

[Blind] - when already in blind.

Resyncs the selected cue to the live selected cue (when blind cue has been changed or when preserve blind cue has been enabled).

 [Params] + [Focus] / [Color] / [Beam]

To expand/suppress categories on displays (Eos and Gio)

 [Data] + [Focus Encoder Page] / [Color Encoder Page] etc

To expand/suppress categories on displays. (Ion)

[Flexi] + [Time]

To invoke flexi time view on displays (All except Element)

[Flexi] + Encoder Paging key

To invoke flexi encoder states

[Shift] + [Label] – maintained press

Toggles the display between default view of referenced data and alternate view.

Keep Shift depressed to page.

[Time] – maintained press

Toggles the display to show discrete timing (Eos and Gio)

Keep Time depressed to page.

[Shift] + [Time]

Toggles the display to show discrete timing (Ion)

Keep Shift depressed to page.

[Displays] + [Level Wheel]

Dim the littlelites or backlighting/LCDs on Gio (as selected by the user) This is the Browser button on Element

[Data] – maintained press

Toggles the display to show data living under referenced data.

Keep Data depressed to page.

[Format] + [Level Wheel]

Zooms the display in focus

[Fader Page] + [Rate Wheel]

Rolls the selected fader page (Eos and Gio)

[Fader Page] + [number]

Select a fader page on integral faders (Eos and Gio)

[Shift] + [Load]

To remove content from a fader

[Fader Controls] + [Bump Button]

Select a fader page on wings

[Shift] + [Select]

Reset Display Columns

[Shift] + [Up], [Shift] + [Down], [Shift] + [Level Wheel]

Resize columns

[Shift] + [Left], [Shift] + [Right]

Move columns

**Operations**

[at] [Enter]

Removes move information from selected channel/parameters. If done in live, posts the value from the previous cue (numeric) manually. If done in blind, allows the value from the previous cue to track in.

[Sneak] [Sneak]

Releases NPs of selected channels and self terminates

[at] [at] – requested change.

Set to Level (Ion, Element)

[Full] [Full]

Sets selected channels intensity to “full” and self terminates

[thru] [thru]

The thru command accesses only the channels displayed in the current flexi-state (unless the channel range specified is NOT in the current display). [Thru] [Thru] selects the range regardless of the flexi mode.

[Undo]

Clears an unterminated command line. Otherwise opens undo controls

[Undo] [Undo]

Posts last undoable command for undo. (Future)

[Shift] + [Sneak]

Makes manual data “unmanual”. It leaves the values as they are, but they are then no longer available for update or record only operations. When executed from an empty command line, this affects all manual data. When done with a channel selection, this affects only those channels.

[Shift] + [Full]

Flash On

[Shift] + [Out]

Flash Out

[Shift] + [+]

+% (Ion and Element)

[Shift] + [-]

-% (Ion and Element)

[Shift] + [Update]

Shortcut to “Save”

[Timing Disable] + [Go]

Cut the next cue

[Timing Disable] + [Back]

Cut the last cue

[Recall From] [Recall From]

Posts Recall From Cue to the command line

 [Select Last] [Select Last]

Repeat last command line, unterminated

[Select Active] [Select Active]

Select Active minus Submaster Contributions

[Shift] + [Select Last]

Posts additional channel selection options to the softkeys

 [Update] + [Sub Bump]

To update a specific submaster

[Label] [Label]

Appended to a record target command, clears the current label, this includes show file labels.

[Shift] + restore manual channel faders.

Reset faders to zero without asserting control.

[Shift] + [Delay]

Posts follow

[Shift] + [Delay] [Delay]

Posts hang (Eos/Gio/Ion)

[Trace] [Trace]

Forces a previously inactive light to track its new intensity setting backwards.

[Shift] + [Encoder Page Key]

Posts the category to the command line (Ion/Gio)

[Shift] + [Parameter]

From the encoder controls, posts the parameter to the command line (Gio)

[Shift] + [Encoder Toggle]

Posts the parameter to the command line (Ion)